**HUNTEX RO-60**

**DISPERSING & LEVELING AGENT**

In high temperature, high speed dyeing conditions, dispersing and leveling agents must to have some required: low-foaming, good dispersion, strong diffusion and retarding effect, etc… Huntex RO-60 is an ideal dispersing leveling agent, suitable in above condition.

**Properties:**

1. Appearance: yellow transparent liquid
2. Component: Particular surfactants
3. pH value: 7 + 1(1% aqueous solution)
4. Ionic nature: Anion/ Nonionic
5. Solubility: Soluble in cold or warm water.

**Features:**

1. HUNTEX RO-60 is a low foam product, suitable to be used for the high-speed and high- pressure dyeing machines.
2. HUNTEX RO-60 have strong diffusing and retarding effect, so If used it in Filament fabric Dyeing batch, we can achieve good levelness.
3. This agent is very economical. The dosage is reduced, because of its high concentrations.
4. The dispersion ability of this product is very good, to prevent precipitation of dyestuffs in high-temperature.
5. HUNTEX RO-60 have strong diffusing and retarding effect, but no effect reproducibility of shading color.

**Usage:**

The amount of use for exhaust process: 0.2 🡪 1.0g/l

**Packaging:**

120kg/ plastic barrel

Expiry date: 3 months.

Note environmental preservation in cool and dry place.