**HUNTEX POS-92**

**SOFTENER FOR BRUSHING PROCESS OF FLEECE FABRIC**

Fleece fabrics are knitted fabrics. At least one side of fabric is brushed to loosen fibers and creat a nap or raised surface for a soft, plush feel. HUNTEX POS-92 is a softening finishing agent for Polyester, Cotton, various their blended fabrics and other synthetic fibers It support for brushing process easily and evenly .

**General trait**

1. Appearance : milky white liquid
2. pH : 5.0 ± 1.0 (25oC, 1% aqueous solution)
3. Ionicity : nonion /cationic
4. Solubility : Soluble in cold water

**Characteristic**

1. HUNTEX POS-92 is suitable for the pre-brushing treatment process of cotton, synthetic fibers and their blends, which can improve the brushing efficiency and reduce the number and time of brushing process.
2. Impart soft and good hand feeling.
3. It can increase the tear strength of the fabric and improve softness hand-feel and anti static ability.
4. High stability to acid, alkali, hard water, etc., does not make yellowing with white fabric , and does not affect shading color and color fastness .
5. Use with resin agent , to give the fiber a moderate luster and a silky touch.

**Instructions**

1. Padding method, recommended dosage: 10g/l 🡪 30g/l
2. Exhaust method, recommended dosage: 1.0% 🡪 5.0% w.o.f .

**Package**

120kg/barrel