**HUNTEX SE-171**

**SCOURING EMULSIFIER**

Huntex SE-171 is souring emulsifier, used in pretreatment process for cotton, T/C fabric. Especially, for saving time, energy, water, this agent can use in dyeing batch. For the knitted cotton fibers, the product not only can be used as the oil emulsifier but also have scouring effect. Especially, in alkali condition, this agent be used will get the best scouring result.

**Properties:**

1. Appearance: White transparent liquid
2. Component: Special surfactants
3. pH value: 7.0 ± 1.0 (25OC ,1% solution)
4. Ionic nature: Non-ionic
5. Solubility: Soluble in cold water or warm water.

**Features:**

1. During the pretreatment and dyeing process, the product is suitable in acid and alkali condition.
2. This agent has an excellent efficiency on scouring process , because it can emulsifier oil knitting , prevent unleveling or spot color .
3. This agent is stable in dyeing process, no effect color shade .

**Usage:**

1. For exhaust Process, the amount of regular use : 1.0g/l 🡪 2.0g/l
2. For continue process, the amount of regular use: 5.0g/l 🡪10g/l

**Packaging:** 120kg/ drums