**HUNTEX HT-411P**

**ANTI-WRINKLE AGENT IN BATH FOR SYNTHETIC FIBER**

HUNTEX HT-411P is the most suitable bath anti-wrinkle agent, suitable with Teteron (polyester), nylon and its blended fiber. It has excellent anti-wrinkle effect and also has the effect of removing oil stains. In high temperature or atmospheric pressure dyeing, HUNTEX HT-411P can effectively prevent wrinkles, creases, scratches, water marks and so on.

**General property**

1. Appearance : white transparent emulsion
2. Ion : Nonionic
3. pH : 7.0 ± 1.0 (25oC, 1% solution)
4. Solubility : Soluble in cold or warm water

**Characteristic**

1. It can improve the hydrophilicity of the fiber in the dye bath, so it can prevent wrinkles, wrinkles and creases, and can improve the elasticity and softness of the fiber.
2. In the dyeing or bleaching process, the oil on the fabric can be removed.
3. High temperature stability, low foaming and good workability.
4. It has good compatibility with various additives and other agents.
5. Does not affect color sleading, leveling and fastness.
6. Good storage stability, no stratification, and no precipitation.
7. After using, It can thick feeling of post processing.

**Instructions**

. Padding method or exhaust process, recommended dosage: 1.0g/l 🡪 2.0g/l

**Package**

120kg/barrel