**HUNTEX SI-T14**

**AMINO SILICONE SOFTENER**

Huntex SI-T14 is a amino silicone softener, designed for use of a premium textile softener. It is applicable for all types of fabric (nature and synthetic fabric). When using it in the finishing process, it increases the soft, smooth, full hand feel and the elasticity of woven and knitted fabric.

**Characteristics**

1. Appearance : Clear white liquid
2. Ionic : Nonionic
3. pH value : 5.0 + 1.0 (1% aq. soln. at 250C）
4. Solubility : Soluble in cold and hot water

**Features**

1. HUNTEX SI-T14 gives outstanding softness with slippery, smooth, full hand fell to all types of fabric. Dilution stability with water.

2. Compatible with organic softeners, durable press resins, optical brighteners and anti-static agents typically co-applied in finishing bath.

3. HUNTEX SI-T14 has a low yellowing degree and it does not discoloration of dyed fabrics

4. HUNTEX SI-T14 gives excellent elasticity to fabric. The elasticity and hand fell of fabric slightly change after many times of washing.

**Application**

The amount of use varies depending on the type of fabric and fiber. The general recommended amount is as follows

1. Exhaustion method , recommended dosage : 0.3% 🡪 1.0% o.w.f
2. Padding method , recommended usage : 3.0g/l 🡪 10g/l

**Packing**

120 Kg/Drum

Storage time: 3 months from production date